VALUES ON THE DIAGNOSIS TOOL

Monitor item | Condition | Value/Status
STOP LAMP SW | Brake pedal: Depressed | On
Brake pedal: Released | Off
ENG SPEED SIG | Engine stopped (Engine speed: Less than 400 rpm) | Stop
Engine running (Engine speed: 400 rpm or more) | Run
ETS ACTUATOR | Engine stopped (Ignition switch: ON) | Off
Engine running | On
4WD WARN LAMP | AWD warning lamp: ON | On
AWD warning lamp: OFF | Off
4WD MODE SW | Always | ##
4WD MODE MON | Engine running | AUTO
DIS-TIRE MONI | Vehicle running with normal size tire installed | 0 – 4 mm
Vehicle running with improper size tire installed (Front/rear tire size difference, wear condition) | 4 – 8 mm, 8 – mm
P BRAKE SW | Parking brake operated | On
Parking brake not operated | Off
BATTERY VOLT | Always | Battery voltage
THRTL POS SEN | When depressing accelerator pedal (Value rises gradually in response to throttle position.) | 0 – 100%
ETS SOLENOID | Engine running

- At idle speed

Approx. 0.000 A
Engine running

- 3,000 rpm or more constant

Approx. 0.000 – 0.500 A*
FR RH SENSOR | Vehicle stopped | 0.00 km/h (0.00 mph)
Vehicle running ■ CAUTION ■ Check air pressure of tire under standard condition. | Approx. equal to the indication on speedometer (Inside of ±10%)
FR LH SENSOR | Vehicle stopped | 0.00 km/h (0.00 mph)
Vehicle running ■ CAUTION ■ Check air pressure of tire under standard condition. | Approx. equal to the indication on speedometer (Inside of ±10%)
RR RH SENSOR | Vehicle stopped | 0.00 km/h (0.00 mph)
Vehicle running ■ CAUTION ■ Check air pressure of tire under standard condition. | Approx. equal to the indication on speedometer (Inside of ±10%)
RR LH SENSOR | Vehicle stopped | 0.00 km/h (0.00 mph)
Vehicle running ■ CAUTION ■ Check air pressure of tire under standard condition. | Approx. equal to the indication on speedometer (Inside of ±10%)
*: The values are changed by throttle opening and engine speed.

TERMINAL LAYOUT
PHYSICAL VALUES

Terminal No. (Wire color) | Description | Condition | Value (Approx.)
+ | - | Signal name | Input/Output
1 (R) | Ground | AWD solenoid power supply | Output | Engine speed: At idle | 2.5 V
Engine speed: 3,000 rpm or more constant | 8 V*
2 (G) | Ground | AWD solenoid ground | — | Engine speed: At idle | 0 V
Engine speed: 3,000 rpm or more constant | 0 V
6 (V) | — | — | — | — | —
7 (W) | Ground | Ignition switch | Input | Ignition switch: ON | Battery voltage
Ignition switch: OFF | 0 V
8 (L) | — | CAN-H | Input/Output | — | —
9 (Y) | Ground | Power supply (AWD solenoid) | Input | Always | Battery voltage
10 (B) | Ground | Ground | — | Always | 0 V
11 (B) | Ground | Ground | — | Always | 0 V
16 (P) | — | CAN-L | Input/Output | — | —
*: The values are changed by throttle opening and engine speed.
■ CAUTION ■
When using circuit tester to measure voltage for inspection, be sure not to extend forcibly any connector terminals.