WORK SUPPORT

Service item | Setting item | Setting
HAZARD ANSWER BACK | Lock Only* | With locking only | Sets the hazard warning lamp answer back function when the door is lock/unlock with the request switch or the key fob.
Unlk Only | With unlocking only
Lock/Unlk | With locking/unlocking
Off | Without the function
*: Factory setting

DATA MONITOR

Monitor item [Unit] | Description
REQ SW-DR [On/Off] | The switch status input from the request switch (driver side)
REQ SW-AS [On/Off] | The switch status input from the request switch (passenger side)
PUSH SW [On/Off] | The switch status input from the push-button ignition switch
TURN SIGNAL R [On/Off] | Each switch condition that BCM judges from the combination switch reading function
TURN SIGNAL L [On/Off]
HAZARD SW [On/Off] | The switch status input from the hazard switch
RKE-LOCK [On/Off] | Lock signal status received from the remote keyless entry receiver
RKE-UNLOCK [On/Off] | Unlock signal status received from the remote keyless entry receiver
RKE-PANIC [On/Off] | Panic alarm signal status received from the remote keyless entry receiver

ACTIVE TEST

Test item | Operation | Description
FLASHER | RH | Outputs the voltage to blink the right side turn signal lamps.
LH | Outputs the voltage to blink the left side turn signal lamps.
Off | Stops the voltage to turn the turn signal lamps OFF.