OUTLINE

- BCM incorporates a power saving control function that reduces the power consumption according to the vehicle status.
- BCM switches the status (control mode) by itself with the power saving control function. It performs the sleep request to each unit (IPDM E/R and combination meter) that operates with the ignition switch OFF.
Normal mode (wake-up)

- CAN communication is normally performed with other units
- Each control with BCM is operating properly

CAN communication sleep mode (CAN sleep)

- CAN transmission is stopped
- Control with BCM only is operating

Low power consumption mode (BCM sleep)

- Low power consumption control is active
- CAN transmission is stopped

LOW POWER CONSUMPTION CONTROL WITH BCM
BCM reduces the power consumption with the following operation in the low power consumption mode.

- The reading interval of the each switches changes from 10 ms interval to 60 ms interval.

Sleep mode activation

- BCM receives the sleep-ready signal (ready) from IPDM E/R and combination meter via CAN communication.
- BCM transmits the sleep wake up signal (sleep) to each unit when all of the CAN sleep conditions are fulfilled.
- Each unit stops the transmission of CAN communication with the sleep wake up signal. BCM is in CAN communication sleep mode.
- BCM is in the low power consumption mode and perform the low power consumption control when all of the BCM sleep conditions are fulfilled with CAN sleep condition.

Sleep condition

CAN sleep condition | BCM sleep condition

- Receiving the sleep-ready signal (ready) from all units
- Ignition switch: OFF
- Vehicle security system and panic alarm: Not operation
- Warning chime: Not operation
- Intelligent Key system buzzer: Not operation
- Trunk room lamp switch status: No change
- Stop lamp switch: OFF
- Key slot (card switch) status: No change
- Turn signal indicator lamp: Not operation
- Exterior lamp: OFF
- Door lock status: No change
- CONSULT-III communication status: Not communication
- Meter display signal: Non-transmission
- Door switch status: No change
- Rear window defogger: OFF

- Interior room lamp battery saver: Time out
- RAP system: OFF
- Push-button ignition switch illumination: OFF
- Nissan Vehicle Immobilizer System (NVIS) - NATS: Not operation
- Remote keyless entry receiver communication status: No communication
- LOCK indicator lamp: OFF
- ACC indicator lamp: OFF
- ON indicator lamp: OFF

Wake-up operation

- BCM changes from the low power consumption mode to the CAN communication sleep mode when the any of the BCM wake-up conditions is fulfilled. Only the control with BCM is activated.
- BCM transmits the sleep wake up signal (wake up) to each unit when any of the CAN wake-up conditions is fulfilled. It changes from the low power consumption mode or the CAN communication sleep mode to the normal mode.
- Each unit starts the transmission of CAN communication with the sleep wake up signal. In addition, the combination meter transmits the wake up signal to BCM via CAN communication to report the CAN communication start.

Wake-up condition

BCM wake-up condition | CAN wake-up condition

- Trunk lid opener switch: OFF → ON
- Remote keyless entry receiver: Receiving
- Door lock and unlock switch:
  NEUTRAL → LOCK, NEUTRAL → UNLOCK

- Receiving the sleep-ready signal (Not-ready) from any units
- Key slot (key switch): OFF → ON, ON → OFF
- Push-button ignition switch (push switch): OFF→ ON
- Hazard switch: OFF → ON
- PASSING switch: OFF → ON, ON → OFF
- TAIL LAMP switch: OFF → ON
- Driver door switch: OFF → ON, ON → OFF
- Passenger door switch: OFF → ON, ON → OFF
- Trunk room lamp switch: OFF → ON, ON → OFF
- Driver door request switch: OFF → ON
- Passenger door request switch: OFF → ON
- Trunk lid request switch: OFF → ON
- Stop lamp switch signal: ON