DTC DETECTION LOGIC

DTC | Self-diagnosis name | DTC detection condition | Possible cause
P0896 | Shift solenoid "E" control circuit high | A DTC is set if the sequence solenoid valve monitor value is ON when the sequence solenoid valve command value is OFF. |

- Sequence solenoid valve
- Harness or connector
  (Open or short in the sequence solenoid valve circuit)

DTC CONFIRMATION PROCEDURE
■ CAUTION ■
Be careful of the driving speed.
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Start the engine.
2. Shift the shift lever to the A position and run at idle for 5 seconds or more.
3. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Start the engine.
2. Shift the shift lever to the A position and run at idle for 5 seconds or more.
3. Check self-diagnosis.

Is DTC P0770 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.