1.CHECK DOOR REQUEST SWITCH

1. Turn ignition switch OFF.
2. Disconnect malfunctioning outside handle connector.
3. Check continuity between malfunctioning outside handle terminals.

Terminal | Condition | Continuity
Outside handle
1 | 2 | Door request switch | Pressed | Existed
Released | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace malfunctioning outside handle. Refer to Removal and Installation (GT-R certified NISSAN dealer).