DTC DETECTION LOGIC

DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
B2616 | Ignition relay circuit | An immediate operation of ignition relay (fuse block) is requested by BCM, but there is no response for more than 1 second |

- Harness or connectors
  (Ignition relay circuit is open or shorted)
- Ignition relay (Fuse block)
- BCM

DTC CONFIRMATION PROCEDURE
1.PERFORM DTC CONFIRMATION PROCEDURE

1. Turn ignition switch ON under the following conditions, and wait for at least 1 second.

- Shift lever is in the P or N position.
- Do not depress brake pedal.

2. Check “Self diagnostic result” with CONSULT-III.

Is DTC detected?
YES>>Go to Diagnosis Procedure.
NO>>INSPECTION END