NOTE： If “WRITE CONFIGURATION” is unsuccessful, perform “Accessory Number Initialization”. For details, refer to On Board Diagnosis Function. After performing “Accessory Number Initialization”, reboot the AV control unit to perform “WRITE CONFIGURATION”.
1.WRITING MODE SELECTION
CONSULT-III Configuration
Select “CONFIGURATION” of “MULTI AV”.
When writing saved data>>GO TO 2.
When writing manually>>GO TO 3.
2.PERFORM “WRITE CONFIGURATION‐CONFIG FILE”
CONSULT-III Configuration
Perform “WRITE CONFIGURATION‐Config file”.
>>WORK END
3.PERFORM “WRITE CONFIGURATION‐MANUAL SELECTION”
CONSULT-III Configuration
Select “WRITE CONFIGURATION-Manual selection” to write vehicle specifications into the AV control unit. For data to write, refer to Configuration List.
>>GO TO 4.
4.OPERATION CHECK
Check that the operation of the AV control unit and camera images (fixed guide lines and predictive course lines) are normal.
>>WORK END