- The clutch A pressure sensor is installed on the front control module and detects the pressure applied to the clutch A.
- The clutch A pressure sensor converts the pressure applied to the clutch A into output voltage and transmits the signal to TCM. TCM uses this signal in calculations for control switching or other functions.
- The clutch A pressure sensor output voltage varies depending on the pressure variations. The voltage increases as the pressure increases.