INSPECTION AFTER INSTALLATION

1.Check shock absorber actuator harness connector (1) for proper connection.

2.Check wheel sensor harness connector for proper connection. Refer to Exploded View (GT-R certified NISSAN dealer).

3.Check wheel alignment. Refer to Adjustment.

4.Adjust neutral position of steering angle sensor. Refer to Special Repair Requirement (GT-R certified NISSAN dealer).

INSPECTION AFTER DISASSEMBLY
Shock Absorber
Check the following items, and replace the part if necessary.

- Shock absorber for deformation, cracks or damage.
- Piston rod for damage, uneven wear or distortion.
- Oil leakage.
- Shock absorber harness connector for damage.

Mount Insulator and Rubber Parts Inspection
Check mount insulator for cracks and rubber parts for wear. Replace it if necessary
Coil Spring
Check coil spring for cracks, wear or damage. Replace it if necessary.