INSPECTION AFTER REMOVAL

- Check each part of steering column assembly for damage or other malfunctions. Replace if necessary.
- Measure steering column assembly rotating torque using a preload gauge [SST: ST3127S000 (J-25765-A)]. Replace steering column assembly if outside the standard.

  Rotating torque | : Refer to Steering Column Operating Range (GT-R certified NISSAN dealer).

- Install the bracket and steering column housing so that the clearance (A) is within the specified range as described below. Replace steering column assembly if out side the standard.

  A | : Refer to Steering Column Mounting Dimensions (GT-R certified NISSAN dealer).

INSPECTION AFTER INSTALLATION

- Check each part of steering column assembly for damage or other malfunctions. Replace if necessary.
- Check the steering wheel play, neutral position steering wheel, steering wheel turning force, and front wheel turning angle. Refer to Inspection.
- Check tilt and telescopic mechanism operating range tilt operating range (L1), telescopic operating range (L2) as shown in the figure.

  L1 | : Refer to Steering Column Operating Range (GT-R certified NISSAN dealer).
  L2 | : Refer to Steering Column Operating Range (GT-R certified NISSAN dealer).