Unit | Description
Combination meter |

- Receives the shift position signal from TCM via CAN communication, and displays the shift position to the shift position indicator.
- Receives the shift position signal from TCM via CAN communication, and if the status does not allow a shift change, it blinks the shift position display in the shift position indicator.

TCM | Transmits the shift position signal to the combination meter via CAN communication.