Abbreviation | Material name | Heat resisting temperature °C (°F) | Resistance to gasoline and solvents | Other cautions
PE | Polyethylene | 60 (140) | Gasoline and most solvents are harmless if applied for a very short time (wipe out quickly). | Flammable
ABS | Acrylonitrile Butadiene Styrene | 80 (176) | Avoid gasoline and solvents. | —
EPM/EPDM | Ethylene Propylene (Diene) copolymer | 80 (176) | Gasoline and most solvents are harmless if applied for a very short time (wipe out quickly). | Flammable
PS | Polystyrene | 80 (176) | Avoid solvents. | Flammable
PVC | Poly Vinyl Chloride | 80 (176) | Gasoline and most solvents are harmless if applied for a very short time (wipe out quickly). | Poisonous gas is emitted when burned.
TPO | Thermoplastic Olefine | 80 (176) | ↑ | Flammable
AAS | Acrylonitrile Acrylic Styrene | 85 (185) | Avoid gasoline and solvents. | —
PMMA | Poly Methyl Methacrylate | 85 (185) | ↑ | —
EVAC | Ethylene Vinyl Acetate | 90 (194) | ↑ | —
PP | Polypropylene | 90 (194) | Gasoline and most solvents are harmless if applied for a very short time (wipe out quickly). | Flammable, avoid battery acid.
PUR | Polyurethane | 90 (194) | Avoid gasoline and solvents. | —
UP | Unsaturated Polyester | 90 (194) | ↑ | Flammable
ASA | Acrylonitrile Styrene Acrylate | 100 (212) | ↑ | Flammable
PPE | Poly Phenylene Ether | 110 (230) | ↑ | —
TPU | Thermoplastic Urethane | 110 (230) | ↑ | —
PBT+ PC | Poly Butylene Terephthalate + Polycarbonate | 120 (248) | ↑ | Flammable
PC | Polycarbonate | 120 (248) | ↑ | —
POM | Poly Oxymethylene | 120 (248) | ↑ | Avoid battery acid.
PA | Polyamide | 140 (284) | ↑ | Avoid immersing in water.
PBT | Poly Butylene Terephthalate | 140 (284) | ↑ | —
PAR | Polyarylate | 180 (356) | ↑ | —
PET | Polyethylene terephthalate | 180 (356) | ↑ | —
PEI | Polyetherimide | 200 (392) | ↑ | —
■ CAUTION ■

- When repairing and painting a portion of the body adjacent to plastic parts, consider their characteristics (influence of heat and solvent) and remove them if necessary or take suitable measures to protect them.
- Plastic parts should be repaired and painted using methods suiting the materials, characteristics.