MOUNTING INSPECTION Check the mounting conditions (looseness, back lash) of each component and component conditions (wear, damage) are normal. WHEEL BEARING INSPECTION

- Move wheel hub and bearing assembly in the axial direction by hand. Check there is no looseness of wheel bearing.

  Axial end play | : Refer to Wheel Bearing (GT-R certified NISSAN dealer).

- Rotate wheel hub, and check that is no unusual noise or other irregular conditions. If there is any of abnormal conditions, replace wheel hub and bearing assembly.