1.CHECK IN-VEHICLE SENSOR

1. Turn the ignition switch OFF.
2. Remove the in-vehicle sensor. Refer to Exploded View.
3. Check the resistance between the in-vehicle sensor terminals. Refer to the applicable table for the normal value.

   Terminal | Condition | Resistance: kΩ
   Temperature: °C (°F)
   1 | 2 | −15 (5) | 12.73
   −10 (14) | 9.92
   −5 (23) | 7.80
   0 (32) | 6.19
   5 (41) | 4.95
   10 (50) | 3.99
   15 (59) | 3.24
   20 (68) | 2.65
   25 (77) | 2.19
   30 (86) | 1.81
   35 (95) | 1.51
   40 (104) | 1.27
   45 (113) | 1.07

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace the in-vehicle sensor.