REMOVAL

1.Remove tires with power tool. Refer to Exploded View.

2.Remove steering knuckle. Refer to Exploded View.

3.Remove stabilizer connecting rod. Refer to Exploded View.

4.Separate shock absorber from transverse link with power tool.

5.Separate shock absorber actuator harness connector (1).

6.Remove shock absorber assembly.
NOTE：
If removing shock absorber is difficult, loosen upper link mounting bolts (vehicle side).

INSTALLATION
Note the following, and install in the reverse order of removal.

- Never pull the shock absorber harness connector.
- Perform final tightening of bolts and nuts at the vehicle installation position (rubber bushing), under unladen conditions with tires on level ground.