DTC DETECTION LOGIC NOTE：

- If DTC B210C is displayed with DTC U1000, first perform the trouble diagnosis for DTC U1000. Refer to DTC Logic.
- When IPDM E/R power supply voltage is low (Approx. 7 - 8 V for about 1 second), the DTC B210C may be detected.

DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
B210C | START CONT RLY OFF | IPDM E/R detects that the relay is stuck in the OFF position even if the followings conditions are met for about 1 second.

- Starter control relay ON/OFF signal from BCM
- P/N position signal from TCM

- IPDM E/R
- Battery

DTC CONFIRMATION PROCEDURE
1.PERFORM DTC CONFIRMATION PROCEDURE

1. Turn the power supply position to start under the following conditions and wait for at least 1 second.

- Shift lever is in the P or N position.
- Do not depress brake pedal.

2. Check “Self diagnostic result” with CONSULT-III.

Is DTC detected?
YES>>Go to Diagnosis Procedure.
NO>>INSPECTION END