1.CHECK POWER POSITION Check if ignition switch position is changing or not. Does ignition switch position change? YES>>GO TO 2. NO>>Check BCM for DTC. Refer to DTC Index.
2.CHECK BUZZER (COMBINATION METER)
Check buzzer (combination meter).
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair or replace the malfunctioning parts.
3.CHECK INTELLIGENT KEY WARNING BUZZER
Check Intelligent Key warning buzzer.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 4.
NO>>Repair or replace the malfunctioning parts.
4.CHECK DOOR SWITCH
Check door switch (driver side).
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 5.
NO>>Repair or replace the malfunctioning parts.
5.CONFIRM THE OPERATION
Confirm the operation again.
Is the result normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.