REMOVAL

1.Turn the ignition switch OFF.

2.Remove instrument lower cover. Refer to Exploded View.

3.Remove the glove box assembly. Refer to Exploded View.

4.Remove instrument lower panel (assist). Refer to Exploded View.

5.Remove the ECM.

6.Disconnect the E-SUS control unit connector.
■ CAUTION ■
Always open the lock lever on the harness connector before disconnecting it.

7.Remove the E-SUS control unit mounting nuts.

8.Remove E-SUS control unit.

INSTALLATION
Install in the reverse order of removal.