1.Adjust parking brake lever stroke. Refer to Inspection and Adjustment.

2.Perform parking brake break-in (drag on) operation by driving vehicle under the following conditions:

- Drive forward
- Vehicle speed: Approx. 40 km/h (25 MPH) set (constant and forward)
- Parking brake operating force: 145 N (15 kg, 33 lb) set contact
- Time: Approx. 10 sec.

■ CAUTION ■

- To prevent lining from getting too hot, allow a cool off period of approximately 5 minutes after every break-in operation.
- Never perform excessive break-in operations, because doing so may cause uneven or early wear of the lining.

3.After the break-in procedure, check parking brake lever stroke of parking brake. Refer to Inspection and Adjustment.