1.CHECK SET-UP SWITCH (SUSPENSION)

1. Turn the ignition switch OFF.
2. Remove the set-up switch (suspension) harness connector.
3. Check the resistance between the set-up switch (suspension) harness connector.

   Set-up switch (suspension) | Resistance
   Terminal | Condition
   6 | 17 | Set-up switch (suspension): Up | Approx. 950 – 1000 – 1050 Ω
   Set-up switch (suspension): Neutral or down | 0 Ω
   24 | 17 | Set-up switch (suspension): Down | Approx. 950 – 1000 – 1050 Ω
   Set-up switch (suspension): Neutral or up | 0 Ω

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace the set-up switch (suspension).