1.CHECK PUSH-BUTTON IGNITION SWITCH ILLUMINATION OPERATION CONSULT-III ACTIVE TEST

1. Turn the ignition switch ON.
2. Select “ENGINE SW ILLUMI” of BCM (INTELLIGENT KEY) active test item.
3. With operating the test items, check that the push-button ignition switch illumination operation.

   On | : Push-button ignition switch illumination ON
   Off | : Push-button ignition switch illumination OFF

Is the push-button ignition switch illumination turned ON/OFF?
YES>>Push-button ignition switch illumination circuit is normal.
NO>>Refer to Diagnosis Procedure.