The actual shapes of Kent-Moore tools may differ from those of special service tools illustrated here.
Tool number (Kent-Moore No.) Tool name |  | Description
KV10116200 (J-26336-A) Valve spring compressor 1. KV10115900 (J-26336-20)
Attachment
2. KV10109220
(　—　)
Adapter
Disassembling valve mechanism
Part (1) is a component of KV10116200 (J-26336-A), but Part (2) is not so.
KV10107902 (J-38959) Valve oil seal puller |  | Replacing valve oil seal
KV10115600 (J-38958) Valve oil seal drift |  | Installing valve oil seal Use side A (G). a: 20 (0.79) dia. d: 8 (0.31) dia. b: 13 (0.51) dia. e: 10.7 (0.421) c: 10.3 (0.406) dia. f: 5 (0.20)
H: side B
Unit: mm (in)
EM03470000 (J-8037) Piston ring compressor |  | Installing piston assembly into cylinder bore
KV10111100 (J-37228) Seal cutter |  | Removing oil pan (lower), front and rear timing chain case, etc.
KV10112100 (BT8653-A) Angle wrench |  | Tightening bolts for connecting rod bearing cap, cylinder head, etc. in angle
KV10111710 (J-3647-A) Heated oxygen sensor wrench |  | Loosening or tightening air fuel ratio sensor 1 For 22 mm (0.87 in) width hexagon nut
KV10114400 (J-38365) Heated oxygen sensor wrench |  | Loosening or tightening heated oxygen senor 2 a: 22 mm (0.87 in)
KV101056S0 (J-49374) Ring gear stopper |  | Fixing flywheel
KV10119100 (J-49360) Resin gasket scraper |  | Liquid gasket scraper for oil pan (upper)