DTC B1210 SIDE COLLISION DETECTION When satellite sensor detects component damage resulting from a side collision, blinks or illuminates the air bag warning lamp to inform the driver. Malfunctioning can be detected by CONSULT-III. OPERATION The front side air bag and side curtain air bag are activated by the air bag diagnosis sensor unit signal transmitted at the time of the side collision.
STRUCTURE
It consists of satellite sensor, air bag diagnosis sensor unit, front side air bag and side curtain air bag.
INSTALLATION
Refer to Exploded View (Front LH/RH side air bag module), Exploded View (Side curtain air bag module), Exploded View (LH/RH satellite sensor).