REMOVAL ■ CAUTION ■ Before removal or installation, always turn the ignition switch OFF and disconnect the battery negative terminal, then wait for at 3 minutes or more.

1.Remove the kicking plate inner and the rear side finisher. Refer to Removal and Installation.

2.Remove the outer anchor.

- Remove the outer anchor cover.
- Remove the outer anchor mounting anchor bolt.

3.Remove the shoulder anchor.

- Remove the shoulder anchor cover.
- Remove the shoulder anchor mounting anchor bolt.

4.Remove the rear pillar finisher. Refer to Removal and Installation.

5.Remove the seat belt pre-tensioner retractor.

- Disconnect the seat belt pre-tensioner connector.
  ■ CAUTION ■
  - To disconnect or connect the seat belt pre-tensioner connector, insert a screwdriver wrapped with tape into the cutout, and raise the lock to disconnect the connector.
  - Connect the connector while raising the lock, and push the lock into the connector.
  - After installing the connector, check that the lock is pushed securely into it.
- Remove the seat belt pre-tensioner retractor mounting anchor bolt and screw.

6.Remove the shoulder anchor bracket. Remove the shoulder anchor bracket mounting bolts.

INSTALLATION
Install in the reverse order of removal.