REMOVAL

1.Fully open the door.

2.Remove the clips (parting seal clip) of door parting seal (1) with the remover tool (A).
■ CAUTION ■
Be careful no to damage the body.

| : Clip

3.Remove the door parting seal from the door assembly.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■
Visually check the clips for deformation and damage at installation. Replace with new ones if necessary.