1.CHECK POWER STEERING SOLENOID VALVE

1. Turn the ignition switch OFF.
2. Disconnect power steering solenoid valve harness connector.
3. Check resistance between power steering solenoid valve connector terminals.

   Power steering solenoid valve | Resistance (Approx.)
   Terminal
   1 | 2 | 4 – 6 Ω

4. Check power steering solenoid valve by listening for its operation sound while applying battery voltage to power steering solenoid valve connector E207 terminals 1 (positive) and 2 (negative).

Is the inspection result normal?
YES >>INSPECTION END
NO>>Replace gear-sub assembly. Refer to Exploded View.