INSPECTION AFTER INSTALLATION

1.Check the engine oil level and add engine oil. Refer to Inspection.
■ CAUTION ■
Be sure to add engine oil before starting engine if drained engine oil from oil cooler.

Oil cooler engine oil capacity | : Approximately 1.3 (1-3/8 us qt, 1-1/8 imp qt)*
*: Engine oil capacity is the reference value.

2.Start the engine, and check there is no leakage of engine oil.

3.Stop the engine and wait for 5 minutes.

4.Check the engine oil level again. Refer to Inspection.