DTC DETECTION LOGIC

DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
P1614 | CHAIN OF IMMU-KEY | Inactive communication between key slot and BCM. |

- Harness or connectors
  (The key slot circuit is open or shorted)
- Key slot
- BCM

DTC CONFIRMATION PROCEDURE
1.PERFORM DTC CONFIRMATION PROCEDURE 1

1. Insert Intelligent Key into the key slot.
2. Check “Self diagnostic result” with CONSULT-III.

Is DTC detected?
YES>>Go to Diagnosis Procedure.
NO>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE 2

1. Press the push-button ignition switch.
2. Check “Self diagnostic result” with CONSULT-III.

Is DTC detected?
YES>>Go to Diagnosis Procedure.
NO>>INSPECTION END