DTC DETECTION LOGIC

DTC | CONSULT‐III display description | DTC Detection Condition | Probable cause
U0415 | VEHICLE SPEED | When the vehicle speed signal received from the ABS actuator and electric unit (control unit) remains abnormal for 2 seconds or more. |

- ABS actuator and electric unit (control unit)
- BCM

DTC CONFIRMATION PROCEDURE
1.DTC CONFIRMATION

1. Erase the DTC.
2. Turn ignition switch OFF.
3. Perform the “Self Diagnostic Result” of CONSULT-III, when passed 2 seconds or more after the ignition switch is turned ON.

Is any DTC detected?
YES>>Refer to Diagnosis Procedure.
NO>>INSPECTION END