1.CHECK ENGINE OIL TEMPERATURE SENSOR

1. Turn ignition switch OFF.
2. Disconnect engine oil temperature sensor harness connector.
3. Remove engine oil temperature sensor.
4. Check resistance between engine oil temperature sensor terminals by heating with hot water as shown in the figure.

   Terminals | Condition | Resistance (kΩ)
   1 and 2 | Temperature　[°C (°F)] | 20 (68) | 2.1 - 2.5
   50 (122) | 0.68 - 1.00
   90 (194) | 0.236 - 0.260

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace engine oil temperature sensor.