1.CHECK STEERING LOCK RELAY Check voltage between IPDM E/R harness connector and ground.

(+) | (–) | Condition | Voltage (V) (Approx.)
IPDM E/R
Connector | Terminal
E5 | 11 | Ground | Ignition switch OFF | A few seconds after opening the driver door | Battery voltage
Ignition switch LOCK | Press the push-button ignition switch | Battery voltage
Ignition switch ACC or ON | 0

Is the inspection normal?
YES>>GO TO 2.
NO>>Replace IPDM E/R. Refer to Removal and Installation.
2.CHECK INTERMITTENT INCIDENT
Refer to Intermittent Incident.
>>INSPECTION END