DTC DETECTION LOGIC NOTE：

- If DTC B261E is displayed with DTC U1000, first perform the trouble diagnosis for DTC U1000. Refer to DTC Logic.
- If DTC B261E is displayed with DTC U1010, first perform the trouble diagnosis for DTC U1010. Refer to DTC Logic.

DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
B261E | VEHICLE TYPE | Difference of BCM configuration | BCM

DTC CONFIRMATION PROCEDURE
1.PERFORM DTC CONFIRMATION PROCEDURE

1. Turn ignition switch ON.
2. Check “Self diagnostic result” with CONSULT-III.

Is DTC detected?
YES>>Go to Diagnosis Procedure.
NO>>INSPECTION END