DTC DETECTION LOGIC

DTC | Display item | Malfunction detected condition | Possible cause
C1164 | CV 1 | When the control unit detects a malfunction in the CV1 system. |

- Harness or connector
- ABS actuator and electric unit (control unit)

C1165 | CV 2 | When the control unit detects a malfunction in the CV2 system.

DTC CONFIRMATION PROCEDURE
1.DTC REPRODUCTION PROCEDURE

1. Turn the ignition switch ON.
2. Perform self-diagnosis for “ABS” with CONSULT-III.

Is DTC “C1164” or “C1165” detected?
YES>>Proceed to diagnosis procedure. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END