REMOVAL

1.Remove heater & cooling unit assembly. Refer to Exploded View (GT-R certified NISSAN dealer).

2.Remove heater pipe bracket and heater pipe grommet.

3.Remove mounting screws (A), and then remove heater pipe cover (1).

4.Remove mounting screws (B), and then remove foot duct (left) (2).

5.Slide heater core (3) to leftward (as shown in the figure).

INSTALLATION
Installation is basically the reverse order of removal.
NOTE：
Refer to Refilling when filling radiator with engine coolant.