REMOVAL

1.Remove the hole covers.

2.Remove the clips connecting the engine under cover and the fender protector (front).

3.Remove the clips (engine undercover rear edge) connected with the engine under cover.

4.Remove the bolts connecting the radiator core support.

5.Remove the bolts connecting the bumper brackets (LH,RH).

6.Remove the bolts connecting the bumper fascia.

7.Pull the engine under cover toward the rear of the vehicle and remove.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- Visually check the clips for deformation and damage at installation. Replace with new ones if necessary.
- Always tighten the mounting bolts to the specified torque.
- Be careful to install the hole cover because it may drop in the cover if it is pressed excessively.