DOOR LOCK FUNCTION Door Lock and Unlock Switch

- The door lock and unlock switch (driver side) is build into power window main switch.
- The door lock and unlock switch (passenger side) is build into power window sub-switch.
- Interlocked with the locking operation of door lock and unlock switch, door lock actuators of all doors and fuel lid lock actuator are locked.
- Interlocked with the unlocking operation of door lock and unlock switch, door lock actuators of all doors and fuel lid lock actuator are unlocked.

KEY REMINDER FUNCTION
When door lock and unlock switch are operated while Intelligent Key is inserted into key slot and any door is open, door locks once but immediately unlocks. This operation prevents Intelligent Key from being left in the vehicle.
AUTOMATIC DOOR LOCK/UNLOCK FUNCTION (LOCK OPERATION)
The interlock door lock function is the function that locks all doors linked with the vehicle speed or shift position. It has 2 types as per the following items.
Vehicle Speed Sensing Auto Door Lock*
All doors are locked when the vehicle speed reaches 24 km/h (15 MPH) or more.
BCM outputs the lock signal to all door lock actuators when it detects that the ignition switch is turned ON, all doors are closed and the vehicle speed received from the combination meter via CAN communication becomes 24 km/h (15 MPH) or more.
P Range Interlock Door Lock
All doors are locked when shifting the selector lever from the P position to any position other than P.
BCM outputs the lock signal to all door lock actuators when it detects that the ignition switch is in the ON position and the shift signal received from the TCM via CAN communication is shifted from the P position to any position other than P.
Setting change of Automatic Door Lock/Unlock Function
The lock operation setting of the automatic door lock/unlock function can be changed.
With CONSULT-III
The ON/OFF switching of the automatic door lock function and the type selection of the automatic door lock/unlock function can be performed at the WORK SUPPORT setting of CONSULT-III.
Without CONSULT- III
The automatic door lock function ON/OFF can be switched by performing the following operation.

1.Close all doors (door switch OFF)

2.Turn ignition switch ON

3.Press and hold the door lock and unlock switch for 5 seconds or more in the lock direction within 20 seconds after turning the ignition switch ON.

4.The switching is complete when the hazard lamp blinks.

OFF → ON | : 2 blinks
ON → OFF | : 1 blink

*: This function is set to ON before delivery.
AUTOMATIC DOOR LOCK/UNLOCK FUNCTION (UNLOCK OPERATION)
The automatic door lock/unlock function is the function that unlocks all doors linked with the key position or shift position. It has 2 types as per the following items.
IGN OFF Interlock Door Unlock*
All doors are unlocked when the power supply position is changed from ON to OFF.
BCM outputs the unlock signal to all door lock actuators when it detects that the power supply position is changed from ignition switch ON to OFF.
P Range Interlock Door Unlock
All doors are unlocked when shifting the selector lever from any position other than the P to P position.
BCM outputs the unlock signal to all door lock actuators when it detects that the ignition switch is in the ON position and the shift signal received from TCM via CAN communication is shifted from any position other than the P to P position.
Setting change of Automatic Door Lock/Unlock Function
The unlock operation setting of the automatic door lock/unlock function can be changed.
With CONSULT- III
The ON/OFF switching of the automatic door lock/unlock function and the type selection of the automatic door lock/unlock function can be performed at the WORK SUPPORT setting of CONSULT-III.
Without CONSULT- III
The automatic door lock/unlock function ON/OFF can be switched by performing the following operation.

1.Close all doors below (door switch OFF)

2.Turn ignition switch ON

3.Press and hold the door lock and unlock switch for 5 seconds or more in the unlock direction within 20 seconds after turning the ignition switch ON.

4.The switching is complete when the hazard lamp blinks.

OFF → ON | : 2 blinks
ON → OFF | : 1 blink

*: This function is set to ON before delivery.