1.CHECK PARKING LAMP OPERATION IPDM E/R AUTO ACTIVE TEST

1. Activate IPDM E/R auto active test. Refer to Diagnosis Description.
2. Check that the parking lamp is turned ON.

CONSULT-III ACTIVE TEST

1. Select "EXTERNAL LAMPS" of IPDM E/R active test item.
2. With operating the test items, check that the parking lamp is turned ON.

   TAIL | : Parking lamp ON
   Off | : Parking lamp OFF

Is the parking lamp turned ON/OFF?
YES>>Parking lamp circuit is normal.
NO>>Refer to Diagnosis Procedure.