REMOVAL

1.Turn the ignition switch OFF.

2.Remove instrument lower cover. Refer to Exploded View.

3.Remove glove box assembly. Refer to Exploded View.

4.Remove instrument lower panel (assist). Refer to Exploded View.

5.Remove power steering control unit screws.

6.Remove power steering control unit (1).

7.Disconnect power steering control unit connector.

INSTALLATION
Install in the reverse order of removal.