If some DTCs are displayed at the same time, perform inspections one by one based on the following priority chart.

Priority | DTC
1 | B2562: LOW VOLTAGE
2 |

- U1000: CAN COMM
- U1010: CONTROL UNIT (CAN)

3 |

- B2190: NATS ANTENNA AMP
- B2191: DIFFERENCE OF KEY
- B2192: ID DISCORD BCM-ECM
- B2193: CHAIN OF BCM-ECM
- B2195: ANTI SCANNING

4 |

- B2013: ID DISCORD BCM-S/L
- B2014: CHAIN OF S/L-BCM
- B2553: IGNITION RELAY
- B2555: STOP LAMP
- B2556: PUSH-BTN IGN SW
- B2557: VEHICLE SPEED
- B2560: STARTER CONT RELAY
- B2601: SHIFT POSITION
- B2602: SHIFT POSITION
- B2603: SHIFT POSI STATUS
- B2604: PNP SW
- B2605: PNP SW
- B2606: S/L RELAY
- B2607: S/L RELAY
- B2608: STARTER RELAY
- B2609: S/L STATUS
- B260A: IGNITION RELAY
- B260B: STEERING LOCK UNIT
- B260C: STEERING LOCK UNIT
- B260D: STEERING LOCK UNIT
- B260F: ENG STATE SIG LOST
- B2612: S/L STATUS
- B2614: ACC RELAY CIRC
- B2615: BLOWER RELAY CIRC
- B2616: IGN RELAY CIRC
- B2617: STARTER RELAY CIRC
- B2618: BCM
- B2619: BCM
- B261A: PUSH-BTN IGN SW
- B261E: VEHICLE TYPE
- B26E9: S/L STATUS
- B26EA: KEY REGISTRATION
- U0415: VEHICLE SPEED SIG

5 |

- B2621: INSIDE ANTENNA
- B2622: INSIDE ANTENNA
- B2623: INSIDE ANTENNA

6 | B26E7: TPMS CAN COMM