TOE-IN Loosen the steering outer socket, and then adjust the length using steering inner socket.

Toe-in | : Refer to Wheel Alignment.

■ CAUTION ■

- Always evenly adjust both toe-in alternately and adjust the difference between the left and right to the standard.
- Always fix the steering inner socket when tightening the steering outer socket.

CAMBER
Loosen the mounting nut of transverse link (1) and front suspension member, and then adjust using adjust bolt (2).

Camber | : Refer to Wheel Alignment.

■ CAUTION ■
Always hold the adjust bolt firmly when tightening nut.
CASTER
Remove the upper link mounting bolts (body side), and then adjust them using the thickness (increasing and decreasing) of shims (A).

Caster | : Refer to Wheel Alignment.

■ CAUTION ■

- Refer to figure for selection of shim.
- Assemble the shims and the rubber bushings while facing the rubber bushings toward the upper link side.

NOTE：
The shims and rubber bushings are fitted on a new vehicle [shim: 3 mm (0.12 in)] are a single unit. However the shims for adjustment and rubber bushings are separated parts. When shim: 6 mm (0.24in) is selected, fix it on one side only.