1.CHECK TRUNK LID OPEN FUNCTION Check trunk lid open function with Intelligent Key. Does trunk lid open with Intelligent Key? YES>>GO TO 2. NO>>Refer to Diagnosis Procedure.
2.CHECK TRUNK LID OPENER REQUEST SWITCH
Check trunk lid opener request switch.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair or replace the malfunctioning parts.
3.CHECK OUTSIDE KEY ANTENNA (REAR BUMPER)
Check outside key antenna (rear bumper).
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 4.
NO>>Repair or replace the malfunctioning parts.
4.check vehicle speed signal
Check combination meter.
Refer to DTC Index.
Is the inspection result normal?
YES>>GO TO 5.
NO>>Repair or replace the malfunctioning parts.
5.CONFIRM THE OPERATION
Confirm the operation again.
Is the result normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.