1.CHECK PARKING BRAKE SWITCH Check that the brake warning lamp in the combination meter turns ON/OFF correctly when operating the parking brake pedal. Is the inspection result normal? YES>>GO TO 2. NO>>Check parking brake switch. Refer to Diagnosis Procedure.
2.CHECK SELF-DIAGNOSIS
Perform self-diagnosis for “ABS” with CONSULT-III.
Is the inspection result normal?
YES>>GO TO 3.
NO>>Check items displayed by self-diagnosis.
3.CHECK COMBINATION METER
Check if the indication and operation of combination meter are normal. Refer to CONSULT-III Function (METER/M&A).
Is the inspection result normal?
YES>>Replace ABS actuator and electric unit (control unit). Refer to Exploded View (GT-R certified NISSAN dealer).
NO>>Repair or replace combination meter.