REPLACEMENT/ADJUSTMENT PROCEDURE NOTE： Replace the filler plug gasket and drain plug with new ones after oil level adjustment.

1.Remove the filler plug () and drain plug, and then fill with the transmission oil until it leaks from the drain hole.

Transmission oil | : Refer to General Specification.

■ CAUTION ■

- Always use the specified transmission oil. In addition, always use the filler after cleaning. If use/mixed use/misuse of the transmission oil other than the specified brand occurs, the original performance cannot be obtained or it may cause serious malfunctions.
- Check that dust does not mix.
- Always use paper towels. Never use waste cloth.

2.Install the filler plug and drain plug. Refer to Exploded View (filler plug), Exploded View (drain plug).

3.Start the engine and select the M range.

4.With depressing the brake pedal, shift the paddle shifter to the N range → M range, 1st gear (wait for 5 seconds) → M range, 2nd gear (wait for 5 seconds) → M range, 1st gear → N range at idle.

5.Stop the engine.

6.Remove the filler plug and drain plug, and then fill with the transmission oil until it leaks from the drain hole.

7.Install the filler plug and drain plug. Refer to Exploded View (filler plug), Exploded View (drain plug).

8.Install the heat insulator.

9.Start the engine and run it at idle. Run the engine until the oil temperature reaches 50°C (122°F) while checking FLUID TEMP in “DATA MONITOR” of CONSULT-III.

10.With depressing the brake pedal, shift the paddle shifter to the N range → M range, 1st gear (wait for 5 seconds) → M range, 2nd gear (wait for 5 seconds) → M range, 1st gear → N range at idle.

11.Stop the engine and wait for 5 minutes.

12.Remove the drain plug. Install the drain plug when the transmission oil begins to drip (1 drop/1 second). Refer to Exploded View.
■ CAUTION ■

- Perform from step 11 to step 12 within 25 minutes.
- Repeat the procedure from step 6 if the transmission oil does not leak from the drain hole.
- Never reuse drain plug.

13.Replace the filler plug gasket with new ones.
■ CAUTION ■
Never reuse filler plug gasket.

14.Install the front diffuser. Refer to Exploded View.

15.Select “OIL TEMP HISTORY RESET” in “WORK SUPPORT” of CONSULT-III.

16.Touch “START” to reset oil temperature history.

REFILL ADJUSTMENT PROCEDURE
NOTE：
Replace the filler plug gasket and drain plug with new ones after oil level adjustment.

1.Remove the front diffuser. Refer to Exploded View.

2.Remove the heat insulator.

3.Start the engine and select the M range.

4.With depressing the brake pedal, shift the paddle shifter to the N range → M range, 1st gear (wait for 5 seconds) → M range, 2nd gear (wait for 5 seconds) → M range, 1st gear → N range at idle.

5.Stop the engine.

6.Remove the filler plug () and drain plug, and then fill with the transmission oil until it leaks from the drain hole.

Transmission oil | : Refer to General Specification.

■ CAUTION ■

- Always use the specified transmission oil. In addition, always use the filler after cleaning. If use/mixed use/misuse of non-specified transmission oil other than the specified brand occurs, the original performance cannot be obtained or it may cause serious malfunctions.
- Check that dust does not mix.
- Always use paper towels. Never use waste cloth.

7.Install the filler plug and drain plug. Refer to Exploded View (filler plug), Exploded View (drain plug).

8.Install the heat insulator.

9.Start the engine and run it at idle. Run the engine until the oil temperature reaches 50°C (122°F) while checking FLUID TEMP in “DATA MONITOR” of CONSULT-III.

10.With depressing the brake pedal, shift the paddle shifter to the N range → M range, 1st gear (wait for 5 seconds) → M range, 2nd gear (wait for 5 seconds) → M range, 1st gear → N range at idle.

11.Stop the engine and wait for 5 minutes.

12.Remove the drain plug. Install the drain plug when the transmission oil begins to drip the drop status (1 drop/1 second). Refer to Exploded View.
■ CAUTION ■

- Perform from step 11 to step 12 within 25 minutes.
- Repeat the procedure from step 6 if the transmission oil does not leak from the drain hole.
- Never reuse drain plug.

13.Replace the filler plug gasket with new ones.
■ CAUTION ■
Never reuse filler plug gasket.

14.Install the front diffuser. Refer to Exploded View.