DTC DETECTION LOGIC

DTC | Display Item | Malfunction detected condition | Possible causes
C1750 | RECEIVER FL | The front LH tire pressure receiver dose not receive a signal. | Tire pressure receiver malfunction
C1751 | RECEIVER FR | The front RH tire pressure receiver dose not receive signal.
C1752 | RECEIVER RR | The rear RH tire pressure receiver dose not receive a signal.
C1753 | RECEIVER RL | The rear LH tire pressure receiver dose not receive a signal.

DTC REPRODUCTION PROCEDURE
1.DTC REPRODUCTION PROCEDURE
With CONSULT-III

1. Drive for 3 minutes at a speed of 40 km/h (25 MPH) or more, then drive normally for 10 minutes.
2. Perform self-diagnosis of the low tire pressure warning control unit.

Is DTC “C1750”, “C1751”, “C1752”, or “C1753” detected?
YES>>Perform trouble diagnosis. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END