■ CAUTION ■

- Before TCM is replaced, the IP characteristics must be extracted, based on the information read out from the malfunctioning TCM. For acquiring the IP characteristic data, refer to “CONSULT-III GT-R TCM CONFIGURATION MANUAL”.
- If no IP characteristic data can be extracted, TCM and the transmission assembly must be replaced as a set.

1. | TCM |  |  |  |
Refer to Components in GI section for the symbols shown in the figure.