DTC DETECTION LOGIC

DTC | Self-diagnosis name | DTC detection condition | Possible cause
P2765 | Input/turbine speed sensor "B" circuit | A DTC is set if the status 1 or 2 below is detected with the sleeve B1 or B2 engaged in an odd number gear.

1. The difference between the actual output shaft speed and the output shaft speed converted from the clutch B speed is 1,000 rpm or more.
2. The difference between the vehicle speed signal (meter) (CAN signal) and the output shaft speed converted from the clutch B speed is 1,000 rpm or more.

- Clutch B speed sensor
- Harness or connector
  (Open or short in the clutch B speed sensor circuit)

DTC CONFIRMATION PROCEDURE
■ CAUTION ■
Be careful of the driving speed.
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Start the engine.
2. Select “RANGE”, “GEAR” and “ENGINE SPEED” in “Data Monitor”.
3. Run the vehicle and maintain the following conditions for 5 seconds or more.

   RANGE | : M
   GEAR | : 3
   ENGINE SPEED | : 2,000 rpm or more

4. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Start the engine.
2. Run the vehicle and maintain the following conditions for 5 seconds or more.

   Shift lever | : M range
   Gear | : 3
   Engine speed | : 2,000 rpm or more

3. Check self-diagnosis.

Is DTC P2765 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.