CALIBRATION OF DECEL G SENSOR ■ CAUTION ■

- To calibrate decel G sensor, always use CONSULT-III.
  (Calibration cannot be done without CONSULT-III)
- Perform the G sensor calibration only with the vehicle parked on level surface.

1.ALIGN THE VEHICLE STATUS
Stop the vehicle with front wheels in the straight-ahead position.
■ CAUTION ■

- Keep all tires inflated to correct pressures. Adjust the tire pressure to the specified pressure value.
- Check that there is specified-load in vehicle other than the driver (or equivalent weight placed in driver′s position).

>>GO TO 2.
2.PERFORM THE CALIBRATION OF DECEL G SENSOR

1. Select “ABS”, “WORK SUPPORT” and “DECEL G SEN CALIBRATION” in order with CONSULT-III.
2. Select “START”.
3. After approximately 10 seconds, select “END”.
4. Turn the ignition switch OFF, then turn it ON again.
   ■ CAUTION ■
   Always perform the above operation.

>> GO TO 3.
3.CHECK DATA MONITOR

1. Run the vehicle with front wheels in the straight-ahead position, then stop.
2. Select “ABS”, “DATA MONITOR” and “DECEL G-SEN” in order with CONSULT-III, and check decel G sensor signal.

   DECEL G-SEN | : ±0.08 G

Is the decel G within the specified range?
YES>>GO TO 4.
NO>>Perform the calibration of decel G sensor again, GO TO 1.
4.ERASE THE SELF-DIAGNOSIS MEMORY
Erase self-diagnosis memories for “ABS” with CONSULT-III. Refer to CONSULT-III Function (GT-R certified NISSAN dealer).
Are the memories erased?
YES>>INSPECTION END
NO>>Check the items indicated by the self-diagnosis.