1.CHECK METER FUSE Check the meter fuse. Refer to Fuse and Fusible Link Arrangement. Is 10A fuse [No.4, located in fuse block (J/B)] normal? YES>>GO TO 3. NO>>GO TO 2.
2.CHECK METER FUSE AGAIN
Replace 10A fuse [No.4, located in fuse block (J/B)] and turn ignition switch ON.
Does the meter fuse blow again?
YES>>Repair or replace the related harness.
NO>>INSPECTION END
3.CHECK HARNESS CONNECTION

1. Check harness connection between air bag diagnosis sensor unit and combination meter.
2. Disconnect air bag diagnosis sensor unit connector and turn ignition switch ON.

Does air bag warning lamp turn ON?
YES>>Replace air bag diagnosis sensor unit. Refer to Exploded View.
NO>>Replace combination meter assembly. Refer to Exploded View.