DTC DETECTION LOGIC

DTC | Display item | Malfunction detected condition | Possible cause
U1010 | CONTROL UNIT (CAN) | Detecting error during the initial diagnosis of CAN controller of low tire pressure warning control unit. | Malfunction of low tire pressure warning control unit

DTC CONFIRMATION PROCEDURE
1.DTC REPRODUCTION PROCEDURE
With CONSULT-III

1. Turn the ignition switch OFF to ON.
2. Perform low tire warning control unit self-diagnosis.

Is DTC “U1010” detected?
YES >>Proceed to trouble diagnosis procedure. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END