1.CHECK POWER WINDOW MAIN SWITCH (DRIVER SIDE)

1. Turn ignition switch OFF.
2. Disconnect power window main switch connector.
3. Check continuity between power window main switch terminals.

(+) | (−) | Condition | Continuity
Power window main switch
Connector | Terminal
D8 | 3 | 2 | Driver side switch | AUTO | Existed
Other than above | Not existed
10 | UP | Existed
Other than above | Not existed
11 | DOWN | Existed
Other than above | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace power window main switch. Refer to Removal and Installation.